**Digital Fabric Strength Tester**

Specifications

* Suitable for tensile testing of light medium and heavy fabrics as per ASTM standards
* Load cell capacity: 1000 kgf
* Variable speed: 50-500 mm/min
* Grip separation: 100-1000 mm
* 3 grips (for holding two inches wide fabric samples) suitable for fabric samples.